IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2017-09-05T11:02:59"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160720_1515(x64) - Exporter 17.0.501.0 - Alternate UI 17.13.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "Polantis_Production" of Organization (no name given)
  Owner history of Person "Polantis_Production" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 3 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Generic - 200mm" | object type "Basic Wall:Generic - 200mm:398" | names: "Basic Wall:Generic - 200mm:309152" | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCSLAB | object type "Floor:Generic 150mm" | FLOOR | names: "Floor:Generic 150mm:309211" | material: layers "Floor:Generic 150mm" ("Default Floor" 150.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Other, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Type 1" | object type "Type 1" | names: "DLB040004-V2:Type 1:368567" | material: materials ("Aluminium Gris", "Aluminium") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Other, Phasing

Types
  IFCWALLTYPE "Basic Wall:Generic - 200mm" | STANDARD | 1 occurrence | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Type 1" | 1 occurrence | material: materials ("Aluminium Gris", "Aluminium") | property sets: Data, Dimensions, General, Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Family and Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Generic 150mm" (IFCLABEL)
    Family and Type = "Floor: Generic 150mm" (IFCLABEL)
    Type = "Floor: Generic 150mm" (IFCLABEL)
    Type Id = "Floor: Generic 150mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "DLB040004-V2: Type 1" (IFCLABEL)
    Family and Type = "DLB040004-V2: Type 1" (IFCLABEL)
    Host Id = "Basic Wall: Generic - 200mm" (IFCLABEL)
    Type = "DLB040004-V2: Type 1" (IFCLABEL)
    Type Id = "DLB040004-V2: Type 1" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family Name = "Floor" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Walls" (IFCLABEL)
    Family Name = "Basic Wall" (IFCTEXT)
  Other: 1 more content on 0 objects not shown
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 1523.0569896154 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 1" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 6. (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 2.99999999999999 (IFCAREAMEASURE) [SQUARE_METRE]
    Elevation at Bottom = -150. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation at Top = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter = 6999.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.449999999999998 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.488067848820581 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00197637666886628 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Radius = 10.3 (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 3 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCSLAB, 1 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Generic - 200mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Generic 150mm" (IFCIDENTIFIER)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Generic 150mm" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Generic - 200mm" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "French manufacturer Delabie is a leader in the European sanitary ware market for non-domestic places. Water controls, solutions for disabled people, sanitary ware, for schools, leisure centres, offices, hospitals, airports…" (IFCTEXT)
    Manufacturer = "DELABIE" (IFCTEXT)
    Model = "TEMPOMIX" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "Time flow shower panel" (IFCTEXT)
    Type Name = "Type 1" (IFCTEXT)
    URL = "http://www.delabie.com" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Type 1" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "DELABIE" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Graphics | properties | on 1 object (1 IFCSLAB) | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Data | properties | on 1 type object
    FlowRate lpm = "6 lpm at 3 bar" (IFCTEXT)
    FlowRate lps = "0.10 lps at 3 bar" (IFCTEXT)
    IntegralAccessoryOptions = "Thermostatic mixing valve" (IFCTEXT)
    Operation = "Time flow mixer" (IFCTEXT)
    WaterSupplyTemperatureMaximum = "55°C-85° (∆50°C : CW/HW)" (IFCTEXT)
  General | properties | on 1 type object
    Category = "Shower panel" (IFCTEXT)
    ManufacturerName = "DELABIE" (IFCTEXT)
    ManufacturerURL = "http://www.delabie.com" (IFCTEXT)
    ProductInformation = "http://www.delabie.com/products/790300" (IFCTEXT)
    Version = "v2" (IFCTEXT)