IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2016-07-05T09:59:23"
Preprocessor: "Autodesk Revit Architecture 2011 - 1.0"
Originating system: "20100326_1700(x64)"
Application: "Autodesk Revit Architecture 2011" version "2011" identifier "Revit" by Organization "Autodesk Revit Architecture 2011"

People and organizations
  Person "Polantis_Production" of Organization (no name given)
  Owner history of Person "Polantis_Production" of Organization (no name given) | application "Autodesk Revit Architecture 2011" version "2011" identifier "Revit" by Organization "Autodesk Revit Architecture 2011" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "Project Number" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level -0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | object type "Basic Wall:Generic - 200mm:398" | names: "Basic Wall:Generic - 200mm:127598" | material: layers "Basic Wall:Generic - 200mm" ("Default Wall" 200.) | property sets: Pset_WallCommon, PSet_Revit_Constraints, PSet_Revit_Phasing, PSet_Revit_Structural, PSet_Revit_Dimensions, PSet_Revit_Type_Construction
          1 x IFCBUILDINGELEMENTPROXY | object type "Type 1" | names: "731003-2-EN:Type 1:Type 1:257916" | property sets: PSet_Revit_Constraints, PSet_Revit_Mechanical, PSet_Revit_Identity Data, PSet_Revit_Phasing, PSet_Revit_Type_Data, PSet_Revit_Type_Other

Property sets
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Basic Wall:Generic - 200mm" (IFCLABEL)
  PSet_Revit_Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = 0 (IFCINTEGER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 632.4655306830795 (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level 1" (IFCLABEL)
  PSet_Revit_Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  PSet_Revit_Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Structural Usage = 0 (IFCINTEGER)
  PSet_Revit_Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 5000000.000000001 (IFCAREAMEASURE) [MILLI SQUARE_METRE]
    Length = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1000000000. (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Name = "Default Domestic Cold Water (Polantis_Production),Default Domestic Hot Water (Polantis_Production)" (IFCLABEL)
    System Type = "Domestic Cold Water,Domestic Hot Water" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "70" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  PSet_Revit_Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCLABEL)
    Project Address = "Enter address here" (IFCLABEL)
    Project Issue Date = "Issue Date" (IFCLABEL)
    Project Name = "Project Name" (IFCLABEL)
    Project Number = "Project Number" (IFCLABEL)
    Project Status = "Project Status" (IFCLABEL)
  PSet_Revit_Type_Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol = "M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  PSet_Revit_Type_Graphics | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  PSet_Revit_Type_Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  PSet_Revit_Type_Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Automatic Room Computation Height = FALSE (IFCBOOLEAN)
    Computation Height = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Radius = 8.300000000000001 (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Type_Construction | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Function = 1 (IFCINTEGER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = 0 (IFCINTEGER)
    Wrapping at Inserts = 0 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
  PSet_Revit_Type_Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "French manufacturer Delabie is a leader in the European sanitary ware market for non-domestic places. Water controls, solutions for disabled people, sanitary ware, for schools, leisure centres, offices, hospitals, airports" (IFCLABEL)
    Manufacturer = "DELABIE" (IFCLABEL)
    Model = "PREMIX COMFORT" (IFCLABEL)
    OmniClass Number = "23.45.00.00" (IFCLABEL)
    OmniClass Title = "Sanitary, Laundry, and Cleaning Equipment" (IFCLABEL)
    Type Comments = "Thermostatic mixing valve" (IFCLABEL)
    URL = "http://www.delabie.com" (IFCLABEL)
  PSet_Revit_Type_Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    FlowRate lpm = "90 lpm at 3 bar" (IFCLABEL)
    FlowRate lps = "1,5 lps at 3 bar" (IFCLABEL)
    IntegralAccessoryOptions = "Mixer, tap, valve" (IFCLABEL)
    Operation = "Group thermostatic mixing valve" (IFCLABEL)
    WaterSupplyTemperatureMaximum = "55°C-85° (?50°C : CW/HW)" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Features = "Group thermostatic mixing valve for mixed water distribution from 32° to 42°C: Anti-scalding safety. Regulation of temperature variations. Non-return valves and filters accessible from the exterior without having to remove the mechanism. Thermal cartridge with no specific lever needed (push-button on the control knob). Interchangeable cartridge with automotive cell. High-resistance chrome-plated brass body DZR. Maximum hot water temperature: 85°C. Differential hot water / mixed water: 15°C mini. Pressure differences at the entrance: 1 bar maximum (0.5 bar recommended). Minimum pressure / maximum: 1 to 10 bar (1 to 5 bar recommended). Left hand side hot water inlet (red ring) and right hand side cold water inlet (blue ring). Mixed water outlet at the top (purple ring). For bottom outlet: unscrew / place lid at the top and outlet connector at the bottom. Maximum temperature limiter, can be adjusted by the installer. Reduced risk of scalding by limiting temperature at the point-of-use. 90 lpm at 3 bar - M1"." (IFCLABEL)
    Finish = "Chrome-plated" (IFCLABEL)
    Grade = "ACS - BELGAQUA - PZH" (IFCLABEL)
    Material = "DZR Brass" (IFCLABEL)
    ModelNumber = "731003" (IFCLABEL)
    Name = "PREMIX COMFORT" (IFCLABEL)
    NominalHeight = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 23. (IFCLENGTHMEASURE) [MILLI METRE]
    SerialNumber = "3456330020787" (IFCLABEL)
    WarrantyDescription = "Any manufacturing defect" (IFCLABEL)
    WarrantyDurationUnit = "10 years" (IFCLABEL)
  PSet_Revit_Type_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Basin, shower" (IFCLABEL)
    ManufacturerName = "DELABIE" (IFCLABEL)
    ManufacturerURL = "http://www.delabie.com" (IFCLABEL)
    ProductInformation = "http://www.delabie.com/products/731003" (IFCLABEL)
    Version = "v1" (IFCLABEL)